**Hardware Required**

* Arduino UNO
* Water level sensor
* Connecting wires

**Pin Configuration**

Water level sensor is provided with three output terminals.

* + stands for        +5V
* – stands for        GND
* S stands for        signal

### ****Circuit Diagram of water level detector****

